<CsoundSynthesizer>
<CsOptions>
; Select audio/midi flags here according to platform
-odac  ;;;realtime audio out
;-iadc    ;;;uncomment -iadc if realtime audio input is needed too
; For Non-realtime ouput leave only the line below:
; -o vco2ift.wav -W ;;; for file output any platform
</CsOptions>
<CsInstruments>

sr = 44100
ksmps = 32
nchnls = 2
0dbfs  = 1

; user defined waveform -2: fixed table size (64), number of partials
; multiplier is 1.4
itmp    ftgen 2, 0, 64, 5, 1, 2, 120, 60, 1, 1, 0.001, 1
ift     vco2init -2, 2, 1.4, 4096, 4096, 2


instr 1

icps = p4
ifn  vco2ift icps, -2, 0.5	;with user defined waveform
print ifn
asig oscili 1, 220, ifn		; (-2), and sr/2 bandwidth
     outs asig, asig

endin
</CsInstruments>
<CsScore>

i 1 0 2 20
i 1 3 2 2000
i 1 6 2 20000

e
</CsScore>
</CsoundSynthesizer>

