atonek
Prev | Orchestra Opcodes and Operators | Next

## atonek

atonek — A hi-pass filter whose transfer functions are the complements of the tonek opcode.

## Description

A hi-pass filter whose transfer functions are the complements of the tonek opcode.

## Syntax

    kres atonek ksig, khp [, iskip]

## Initialization

iskip (optional, default=0) -- initial disposition of internal data space. Since filtering incorporates a feedback loop of previous output, the initial status of the storage space used is significant. A zero value will clear the space; a non-zero value will allow previous information to remain. The default value is 0.

## Performance

kres -- the output signal at control-rate.

ksig -- the input signal at control-rate.

khp -- the response curve's half-power point, in Hertz. Half power is defined as peak power / root 2.

atonek is a filter whose transfer functions is the complement of tonek. atonek is thus a form of high-pass filter whose transfer functions represent the “filtered out” aspects of their complements. However, power scaling is not normalized in atonek but remains the true complement of the corresponding unit.

## Examples

Here is an example of the atonek opcode. It uses the file atonek.csd.

Example 59. Example of the atonek opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac     ;;;RT audio out
    ;-iadc    ;;;uncomment -iadc if RT audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o atonek.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>
    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs = 1

    gisin ftgen 0, 0, 2^10, 10, 1

    instr 1

    ksig	randomh	400, 1800, 150
    aout	poscil	.2, 1000+ksig, gisin
    	outs	aout, aout
    endin

    instr 2

    ksig	randomh	400, 1800, 150
    khp	line	1, p3, 400	;vary high-pass
    ksig	atonek	ksig, khp
    aout	poscil	.2, 1000+ksig, gisin
    	outs	aout, aout
    endin

    </CsInstruments>
    <CsScore>
    i 1 0 5
    i 2 5.5 5
    e
    </CsScore>
    </CsoundSynthesizer>

## See Also

areson, aresonk, atone, port, portk, reson, resonk, tone, tonek

## Credits

Author: Robin Whittle
Australia
May 1997

Prev | Up | Next
atone | Home | atonex