beadsynt
Prev | Orchestra Opcodes and Operators | Next

## beadsynt

beadsynt — Band-Enhanced Oscillator-Bank

## Description

Plugin opcode in beosc.

Band-Enhanced oscillator-bank, a port of Loris' oscillator (based on Supercollider's Beadsynt). Can work both with arrays and tables. The band-enhanced family of opcodes (beosc, beadsynt) implement sound modeling and synthesis that preserves the elegance and malleability of a sinusoidal model, while accommodating sounds with noisy (non-sinusoidal) components. Analysis is done offline, with an enhanced McAulay-Quatieri (MQ) style analysis that extracts bandwidth information in addition to the sinusoidal parameters for each partial. To produce noisy components, we synthesize with sine wave oscillators that have been modified to allow the introduction of variable bandwidth.

The synthesis can be controlled via a set of flags (see iflags), allowing to switch between unifrom or gaussian noise for the noise components, wavetable interpolation (switch off to save cpu), and freq. interpolation between k-cycles (switch off to save cpu)

| Note
The original implementation (Loris) uses gaussian (normal) noise for the non-sinusoidal components, which if implemented naively, as in loris, is very cpu intensive. The supercollider port uses simple uniform noise. We implement both, with a very efficient implementation of gaussian noise (using a precomputed table), which makes it as efficient as uniform noise.

## Syntax

    aout beadsynt kFreqs[], kAmps[], kBws[] \
                       [, inumosc, iflags, kfreq, kbw, ifn, iphs ]

    aout beadsynt ifreqft, iampft, ibwft, inumosc \
                       [, iflags, kfreq, kbw, ifn, iphs ]

## Initialization

ifreqft - A table holding the frequencies for each partial

iampft - A table holding the amplitudes for each partial

ibwft - A table holding the bandwidths for each partial

inumosc - the number of partials to resynthesize. In the array case, it can be left unset.

iflags - 0: uniform noise, 1:gaussian noise, +2: oscil linear interpolation, +4: freq. interpolation (default=1)

ifn - A table holding a sine wave (or -1 to use the builtin table) (default = -1)

iphs - Initial phase. -1: randomized, 0-1: initial phase, >1: table number holding the phases (default = -1)

## Performance

aout - The generated sound

kFreqs[] - An array holding the frequencies of each partial

kAmps[] - An array holding the amplitudes of each partial

kBws[] - An array holding the bandwidths of each partial

kfreq - Freq. scaling, all frequencies are multiplied by this (default = 1)

kbw - Bandwidth scaling, all bandwidths are multiplied by this (default = 1)

| Note
`kFreqs[]`, `kAmps[]` and `kBws[]` must all be the same size (this also holds true for `ifreqft`, `iampft` and `ibwft`)

## Examples

Here is an example of the beadsynt opcode. It uses the file beadsynt.csd.

Example 88. Example of the beadsynt opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    -odac
    </CsOptions>
    <CsInstruments>

    /*

    This is the example file for beadsynt

    beadsynt
    ========

    Band-enhanced additive synthesis.
    A port of Loris' band-enhanced resynthesis algorithms
    (basen on Supercollider's BEOsc)

    The band-enhanced family of opcodes (beosc, beadsynt) implement
    sound modeling and synthesis that preserves the elegance and
    malleability of a sinusoidal model, while accommodating sounds
    with noisy (non-sinusoidal) components. Analysis is done offline,
    with an enhanced McAulay-Quatieri (MQ) style analysis that extracts
    bandwidth information in addition to the sinusoidal parameters for
    each partial. To produce noisy components, we synthesize with sine
    wave oscillators that have been modified to allow the introduction
    of variable bandwidth.

    Syntax
    ======

    beadsynt exists in two forms, one using arrays, the other using f-tables

    aout beadsynt kFreqs[], kAmps[], kBws[], inumosc=-1, iflags=1, kfreq=1, kbw=1, ifn=-1, iphs=-1
    aout beadsynt ifreqft, iampft, ibwft, inumosc, iflags=1, kfreq=1, kbw=1, ifn=-1, iphs=-1

    kFreqs[]: an array holding the frequencies of each partial
    kAmps[]: an array holding the amplitudes of each partial
    kBws[]: an array holding the bandwidths of each partial
    ifreqft: a table holding the frequencies of each partial
    iampft: a table holding the amplitudes of each partial
    ibwft: a table holding the bandwidths of each partial
    inumosc: the number of partials to resynthesize (-1 to synthesize all)
    iflags: 0: uniform noise
            1: gaussian noise
           +2: use linear interpolation for the oscil (similar to oscili)
           +4: freq interpolation
    kfreq: freq. scaling factor
    kbw: bandwidth scaling factor
    ifn: a table holding a sine wave (or -1 to use builtin sine)
    iphs: initial phase of the oscillators.
          -1: randomize phase (default)
         0-1: initial phase
         >=1: table holding the phase for each oscillator (size>=inumosc)

    NB: kFreqs, kAmps and kBws must all be the same size (this also holds true for
        ifreqft, iampfr and ibwft)

    This example uses the analysis file fox.mtx.wav which was produced with
    loristrck_pack, see https://github.com/gesellkammer/loristrck

    */

    sr = 44100
    ksmps = 128
    nchnls = 2
    0dbfs = 1.0

    gispectrum ftgen 0, 0, 0, -1, "fox.mtx.wav", 0, 0, 0

    instr 1
      ifn = gispectrum
      iskip      tab_i 0, ifn
      idt        tab_i 1, ifn
      inumcols   tab_i 2, ifn
      inumrows   tab_i 3, ifn
      itimestart tab_i 4, ifn
      inumpartials = inumcols / 3
      imaxrow = inumrows - 2
      it = ksmps / sr
      igain init 1
      ispeed init 1
      idur = imaxrow * idt / ispeed
      kGains[] init inumpartials
      kfilter init 0
      ifreqscale init 1

      kt timeinsts
      kplayhead = phasor:k(ispeed/idur)*idur
      krow = kplayhead / idt
      kF[] getrowlin krow, ifn, inumcols, iskip, 0, 0, 3
      kA[] getrowlin krow, ifn, inumcols, iskip, 1, 0, 3
      kB[] getrowlin krow, ifn, inumcols, iskip, 2, 0, 3

      if(kt > idur*0.5) then
        kfilter = 1
      endif

      if (kfilter == 1) then
        kGains bpf kF, 300, 0.001, 400, 1, 1000, 1, 1100, 0.001
        kA *= kGains
      endif

      iflags = 0    ; uniform noise, no interpolation
      aout beadsynt kF, kA, kB, -1, iflags, ifreqscale

      if(kt > idur) then
        event "e", 0, 0, 0
      endif
      aenv cosseg 0, 0.02, igain, idur-0.02-0.1, igain, 0.1, 0
      aout *= aenv
      outs aout, aout
    endin

    schedule 1, 0, -1

    </CsInstruments>
    <CsScore>
    </CsScore>
    </CsoundSynthesizer>

## See Also

beosc, adsynt2,

## Credits

By: Eduardo Moguillansky 2018

New plugin in version 6.12

Prev | Up | Next
bbcuts | Home | beosc