pvs2tab
Prev | Orchestra Opcodes and Operators | Next

## pvs2tab

pvs2tab — Copies spectral data to k-rate arrays (or t-variables). Also known as pvs2array.

## Description

Copies a pvs frame to a t-variable. Currently only AMP+FREQ and AMP+PHASE formats allowed. Since t-vars are an earlier version of k-rate arrays, the opcode also works with these. The opcode pvs2array is an alias of this one.

## Syntax

    kframe pvs2tab tvar|kvar[], fsig

    kframe pvs2tab kmags[], kfreqs[], fsig

## Performance

kframe -- current copied frame number. It can be used to detect when a new frame has been copied.

tvar|kvar[] -- t-variable or k-rate array containing the output. It is produced at every k-period, but may not contain a new frame, pvs frames are produced at their own frame rate that is independent of kr. Generally, this vector needs to be big enough to contain the frame samples, i.e. N+2 (N is the dft size). If smaller, only a portion of the frame will be copied; if bigger, unused points will exist at higher indexes.

kmags[], kfreqs[] k-rate arrays containing magnitude and frequency values. These arrays need to be generally be of size N/2 + 1, where N is dft frame size. If smaller, only a portion of the pvs frame will be copied; if bigger, unused points will exist at higher indexes.

fsig -- input fsig to be copied.

## Examples

Example 803. Example

    karr[] init 1026
    a1 inch 1
    fsig1   pvsanal a1, 1024,256,1024, 1
    kframe  pvs2tabkarr, fsig1

## Credits

Author: Victor Lazzarini
October 2011

New plugin in version 5

October 2011.

Prev | Up | Next
pvswarp | Home | pyassign Opcodes