GEN24
Prev | Score Statements and GEN Routines | Next

## GEN24

GEN24 — Reads numeric values from another allocated function-table and rescales them.

## Description

This subroutine reads numeric values from another allocated function-table and rescales them according to the max and min values given by the user.

## Syntax

    f # time size -24 ftable min max

## Initialization

#, time, size -- the usual GEN parameters. See f statement.

ftable -- ftable must be an already allocated table with the same size as this function.

min, max -- the rescaling range.

| Note
This GEN is useful, for example, to eliminate the starting offset in exponential segments allowing a real starting from zero.

## Examples

Here is an example of the GEN24 opcode. It uses the file gen24.csd.

Example 1217. Example of the GEN24 generator.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac  ;;;realtime audio out
    ;-iadc    ;;;uncomment -iadc if realtime audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o gen24.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs  = 1

    instr 1

    ifn  = p4				;choose between tables
    kcps init 1/p3				;create index over duration of note.
    kndx phasor kcps
    ixmode = 1				;normalize to 0-1
    kval table kndx, ifn, ixmode
    asig poscil .7, 440 + kval, 1		;add to frequency
         outs asig, asig

    endin
    </CsInstruments>
    <CsScore>
    f 1 0 16384 10 1	;sine wave
    f 10 0 16384 -24 1 0 400;scale sine wave from table 1 from 0 to 400
    f 11 0 16384 -24 1 0 50	;and from 0 to 50

    i 1 0 3 10
    i 1 4 3 11
    e
    </CsScore>
    </CsoundSynthesizer>

## Credits

Author: Gabriel Maldonado

New in Csound version 4.16

Prev | Up | Next
GEN23 | Home | GEN25