getrowlin
Prev | Orchestra Opcodes and Operators | Next

## getrowlin

getrowlin — Copy a row from a 2D array or table, with interpolation between rows

## Description

Plugin opcode in beosc.

Given a 2D array (i- or k- array), or a table representing a 2D matrix, get a row of this matrix (possibly a slice). If krow is not an integer, the values are the result of the interpolation between the two adjacent rows. Assuming such a 2D matrix containing multiple rows of sampled streams (for instance, the amplitudes of a set of oscillators, sampled at a regular interval), this opcode extracts one row of that data with linear interpolation between adjacent rows (if the row is not a round number) and places the result in a 1D array

## Syntax

    kOut[] getrowlin kMtx[], krow [, kstart, kend, kstep ]

    kOut[] getrowlin krow, ifn, inumcols [, iskip, start, iend, istep ]

## Initialization / Performance

kMtrx[] - a 2D array

krow - the row to read (can be a fractional number, in which case interpolation with the next row is performed)

kstart - start index to read from the row (default = 0)

kend - end index to read from the row (not inclusive)

kstep - step used to read the along the row (default = 1)

iskip - in the case of using a table as input, iskip indicates the start of the sampled data (skipping a possible header in the data) (default = 0)

inumcols - in the case of using a table as input, inumcols indicates the number of columns of the 2D matrix.

## Examples

Here is an example of the getrowlin opcode. It uses the file getrowlin.csd. See also the example for beadsynt: beadsynt.csd

Example 398. Example of the getrowlin opcode.

    <CsoundSynthesizer>
    <CsOptions>
    -odac     ;;;realtime audio out
    </CsOptions>
    <CsInstruments>

    /*

    This is the example file for getrowlin

    getrowlin
    =========

      Given a 2D array (i- or k- array), or a table representing a
      2D matrix, get a row of this matrix (possibly a slice). If krow is
      not an integer, the values are the result of the interpolation
      between the two adjacent rows.

      Assuming such a 2D matrix containing multiple rows of sampled streams
      (for instance, the amplitudes of a set of oscillators, sampled at a
      regular interval), this opcode extracts one row of that data with
      linear interpolation between adjacent rows and places the result in
      a 1D array

      NB: The destination array (the left hand term) does not
          need to be previously initialized

      NB2: if the destination array is too small to fit the data, it will
           be enlarged

    Syntax
    ======

    kOut[] getrowlin kMtrx[], krow, kstart=0, kend=0, kstep=1
    kOut[] getrowlin krow, ifn, inumcols, iskip=0, istart=0, iend=0, istep=1

    kMtrx[]  : a 2D array
    krow     : the row to read (can be a fractional number, in which case interpolation
               with the next row is performed)
    kstart   : start index to read from the row
    kend     : end index to read from the row (not inclusive)
    kstep    : step used to read the along the row
    iskip    : in the case of using a table as input, iskip indicates the start of the
               sampled data (skipping a possible header in the data)
    inumcols : in the case of using a table as input, inumcols indicates the number of
               columns of the 2D matrix.

    */

    sr = 44100
    ksmps = 128
    nchnls = 1
    0dbfs  = 1

    ; just a simple test of the bare functionality
    instr 1
      ; make a 4x3 array
      kMtx[] init 3, 4
      kMtx fillarray  0,  1,  2,  3,   \
                     10, 11, 12, 13,   \
                     20, 21, 22, 23
      krow linseg 0, p3, 2
      printk2 krow, 20
      kOut[] getrowlin kMtx, krow
      printarray kOut, -1, "", "kOut"

      ; the same, but use cosine interpolation
      krow0 = floor(krow)
      krow1 = krow0 + 1
      krowcos = lincos(krow, krow0, krow1, krow0, krow1)
      kOut2[] getrowlin kMtx, krowcos
      printarray kOut2, -1, "", "kOut2"
    endin

    ; simplified example taken from beadsynt, to show a practical use case
    ; this uses the file fox.mtx.wav, which is not a real soundfile, but
    ; a 2D matrix saved as a soundfile, generated with loristrck_pack
    ; (see https://github.com/gesellkammer/loristrck)
    instr 2
      ifn ftgentmp 0,0,0,-1, "fox.mtx.wav", 0, 0, 0
      ; ifn is organized as follow:
      ; header: iskip, idt, inumcols, inumrows, itimestart
      ; multiple rows of the form f0, a0, bw0, f1, a1, bw1, ...
      iskip      tab_i 0, ifn
      idt        tab_i 1, ifn
      inumcols   tab_i 2, ifn
      inumrows   tab_i 3, ifn
      itimestart tab_i 4, ifn
      inumpartials = inumcols / 3
      imaxrow = inumrows - 2
      idur = inumrows * idt
      kfreqscale cosseg 1, idur, 2
      kplayhead  phasor (1/idur)*idur
      krow = limit(kplayhead / idt, 0, imaxrow)
      ;                                              start end step
      kFreqs[] getrowlin krow, ifn, inumcols, iskip, 0,    0,  3
      kAmps[]  getrowlin krow, ifn, inumcols, iskip, 1,    0,  3
      kBws[]   getrowlin krow, ifn, inumcols, iskip, 2,    0,  3
      aout beadsynt kFreqs, kAmps, kBws, -1, 0, kfreqscale
      outch 1, aout
      if(timeinsts() > idur) then
        event "e", 0, 0, 0
      endif
    endin

    </CsInstruments>
    <CsScore>
    i 1 0 2
    i 2 2 3600
    </CsScore>
    </CsoundSynthesizer>

## See Also

tabrowlin, beadsynt, getrow, slicearray, copyf2array, tab2array, ftslice,

## Credits

By: Eduardo Moguillansky 2018

New plugin in version 6.12

Prev | Up | Next
getrow | Home | getseed