STKMandolin
Prev | Orchestra Opcodes and Operators | Next

## STKMandolin

STKMandolin — STKMandolin produces mamdolin-like sounds.

## Description

Plugin opcode in stkopd.

STKMandolin produces mamdolin-like sounds, using "commuted synthesis" techniques to model a mandolin instrument.

## Syntax

    asignal STKMandolin ifrequency, iamplitude, [kbody, kv1[, kpos, kv2[, ksus, kv3[, kdetune, kv4[, kmic, kv5]]]]]

## Initialization

ifrequency -- Frequency of note played, in Hertz.

iamplitude -- Amplitude of note played (range 0-1).

## Performance

kbody -- controller 2, size of body. Value range of kv1 is 0-127.

kpos -- controller 4, pluck position. Value range of kv2 is 0-127.

ksus -- controller 11, string sustain. Value range of kv3 is 0-127.

kdetune -- controller 1, string detuning. Value range of kv4 is 0-127.

kmic -- controller 128, position of microphone. Value range of kv5 is 0-127.

| Note
The code for this opcode is taken directly from the Mandolin class in the Synthesis Toolkit in C++ by Perry R. Cook and Gary P. Scavone. More on the STK classes can be found here: https://ccrma.stanford.edu/software/stk/classes.html kc1, kv1, kc2, kv2, kc3, kv3, kc4, kv4, kc5, kv5, kc6, kv6, kc7, kv7, kc8, kv8 -- Up to 8 optional k-rate controller pairs for the STK opcodes. Each controller pair consists of a controller number (kc) followed by a controller value (kv). Both the controller numbers and the controller values are krate variables. However, during a performance, normally the controller numbers stay fixed while the corresponding controller values may change at any time. The order of the controller pair is arbitrary, as long as they are after iamplitude. Also, it is not needed that all controller pairs are used.

## Examples

Here is an example of the STKMandolin opcode. It uses the file STKMandolin.csd.

Example 951. Example of the STKMandolin opcode.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac     ;;;realtime audio out
    ;-iadc    ;;;uncomment -iadc if RT audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o STKMandolin.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs  = 1

    instr 1

    ifrq	=	p4
    kv1	line	p5, p3, p6			;body size
    kv3	=	p7				;sustain

    asig	STKMandolin cpspch(ifrq), 1, 2, kv1, 4, 10, 11, kv3, 1, 100, 128, 100
    	outs asig, asig
    endin

    </CsInstruments>
    <CsScore>

    i 1 0 .3 7.00 100 0 20
    i 1 + .  8.00 10 100 20
    i 1 + .  8.00 100 0 120
    i 1 + 4  8.00 10 10 127
    e
    </CsScore>
    </CsoundSynthesizer>

## See Also

STKPlucked.

## Credits

Author: Michael Gogins (after Perry Cook)
Irreducible Productions
New York, NY

New in Csound version 5.11

Prev | Up | Next
STKHevyMetl | Home | STKModalBar