FLtabs
Prev | Orchestra Opcodes and Operators | Next

## FLtabs

FLtabs — Creates a tabbed FLTK interface.

## Description

FLtabs is a “file card tabs” interface that is useful to display several areas containing widgets in the same windows, alternatively. It must be used together with FLgroup, another container that groups child widgets.

## Syntax

    FLtabs iwidth, iheight, ix, iy

## Initialization

iwidth -- width of widget.

iheight -- height of widget.

ix -- horizontal position of upper left corner of the valuator, relative to the upper left corner of corresponding window. Expressed in pixels.

iy -- vertical position of upper left corner of the valuator, relative to the upper left corner of corresponding window. Expressed in pixels.

## Performance

Containers are useful to format the graphic appearance of the widgets. The most important container is FLpanel, that actually creates a window. It can be filled with other containers and/or valuators or other kinds of widgets.

There are no k-rate arguments in containers.

FLtabs is a “file card tabs” interface that is useful to display several alternate areas containing widgets in the same window.

FLtabs.

It must be used together with FLgroup, another FLTK container opcode that groups child widgets.

## Examples

The following example code:

             FLpanel  "Panel1", 450, 550, 100, 100
             FLscroll 450, 550, 0, 0
             FLtabs   400, 550, 5, 5

             FLgroup  "sliders", 380, 500, 10, 40, 1
    gk1, ihs FLslider  "FLslider 1", 500, 1000, 2 ,1, -1, 300,15, 20,50
    gk2, ihs FLslider  "FLslider 2", 300, 5000, 2 ,3, -1, 300,15, 20,100
    gk3, ihs FLslider  "FLslider 3", 350, 1000, 2 ,5, -1, 300,15, 20,150
    gk4, ihs FLslider  "FLslider 4", 250, 5000, 1 ,11, -1, 300,30, 20,200
    gk5, ihs FLslider  "FLslider 5", 220, 8000, 2 ,1, -1, 300,15, 20,250
    gk6, ihs FLslider  "FLslider 6", 1, 5000, 1 ,13, -1, 300,15, 20,300
    gk7, ihs FLslider  "FLslider 7", 870, 5000, 1 ,15, -1, 300,30, 20,350
    gk8, ihs FLslider  "FLslider 8", 20, 20000, 2 ,6, -1, 30,400, 350,50
             FLgroupEnd

             FLgroup  "rollers", 380, 500, 10, 30, 2
    gk1, ihr FLroller  "FLroller 1", 50, 1000,.1,2 ,1 ,-1, 200,22, 20,50
    gk2, ihr FLroller  "FLroller 2", 80, 5000,1,2 ,1 ,-1, 200,22, 20,100
    gk3, ihr FLroller  "FLroller 3", 50, 1000,.1,2 ,1 ,-1, 200,22, 20,150
    gk4, ihr FLroller  "FLroller 4", 80, 5000,1,2 ,1 ,-1, 200,22, 20,200
    gk5, ihr FLroller  "FLroller 5", 50, 1000,.1,2 ,1 ,-1, 200,22, 20,250
    gk6, ihr FLroller  "FLroller 6", 80, 5000,1,2 ,1 ,-1, 200,22, 20,300
    gk7, ihr FLroller  "FLroller 7",50, 5000,1,1 ,2 ,-1, 30,300, 280,50
             FLgroupEnd

             FLgroup "joysticks", 380, 500, 10, 40, 3
    gk1, gk2, ihj1, ihj2 FLjoy "FLjoy", 50, 18000, 50, 18000, 2, 2, -1, -1, 300, 300, 30, 60
             FLgroupEnd

             FLtabsEnd
             FLscrollEnd
             FLpanelEnd

...will produce the following result:

FLtabs example, sliders tab.

FLtabs example, rollers tab.

FLtabs example, joysticks tab.

(Each picture shows a different tab selection inside the same window.)

## Examples

Here is an example of the FLtabs opcode. It uses the file FLtabs.csd.

Example 318. Example of the FLtabs opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    ; Audio out   Audio in    No messages
    -odac           -iadc     -d     ;;;RT audio I/O
    ; For Non-realtime ouput leave only the line below:
    ; -o FLtabs.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    ; A single oscillator with frequency, amplitude and
    ; panning controls on separate file tab cards
    sr = 44100
    kr = 441
    ksmps = 100
    nchnls = 2

    FLpanel "Tabs", 300, 350, 100, 100
    itabswidth = 280
    itabsheight = 330
    ix = 5
    iy = 5
    FLtabs itabswidth,itabsheight, ix,iy

        itab1width = 280
        itab1height = 300
        itab1x = 10
        itab1y = 40
        FLgroup "Tab 1", itab1width, itab1height, itab1x, itab1y
            gkfreq, i1 FLknob "Frequency", 200, 5000, -1, 1, -1, 70, 70, 130
            FLsetVal_i 400, i1
        FLgroupEnd

        itab2width = 280
        itab2height = 300
        itab2x = 10
        itab2y = 40
        FLgroup "Tab 2", itab2width, itab2height, itab2x, itab2y
            gkamp, i2 FLknob "Amplitude", 0, 15000, 0, 1, -1, 70, 70, 130
            FLsetVal_i 15000, i2
        FLgroupEnd

        itab3width = 280
        itab3height = 300
        itab3x = 10
        itab3y = 40
        FLgroup "Tab 3", itab3width, itab3height, itab3x, itab3y
            gkpan, i3 FLknob "Pan position", 0, 1, 0, 1, -1, 70, 70, 130
            FLsetVal_i 0.5, i3
        FLgroupEnd
    FLtabsEnd
    FLpanelEnd
    ; Run the widget thread!
    FLrun

    instr 1
        ifn = 1
        asig oscili gkamp, gkfreq, ifn
        outs asig*(1-gkpan), asig*gkpan
    endin

    </CsInstruments>
    <CsScore>

    ; Function table that defines a single cycle
    ; of a sine wave.
    f 1 0 1024 10 1

    ; Instrument 1 will play a note for 1 hour.
    i 1 0 3600
    e

    </CsScore>
    </CsoundSynthesizer>

## See Also

FLgroup, FLgroupEnd, FLpack, FLpackEnd, FLpanel, FLpanelEnd, FLscroll, FLscrollEnd, FLtabsEnd

## Credits

Author: Gabriel Maldonado

New in version 4.22

Example written by Iain McCurdy, edited by Kevin Conder.

Prev | Up | Next
FLslider | Home | FLtabsEnd