outrg
Prev | Orchestra Opcodes and Operators | Next

## outrg

outrg — Allow output to a range of adjacent audio channels on the audio output device

## Description

outrg outputs audio to a range of adjacent audio channels on the audio output device.

## Syntax

    outrg kstart, aout1 [,aout2, aout3, ..., aoutN]

## Performance

kstart - the number of the first channel of the output device to be accessed (channel numbers starts with 1, which is the first channel)

aout1, aout2, ... aoutN - the arguments containing the audio to be output to the corresponding output channels.

outrg allows to output a range of adjacent channels to the output device. kstart indicates the first channel to be accessed (channel 1 is the first channel). The user must be sure that the number obtained by summing kstart plus the number of accessed channels -1 is <= nchnls.

## Examples

Here is an example of the outrg opcode. It uses the file outrg.csd.

Example 667. Example of the outrg opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac    ;;;realtime audio out
    ;-iadc    ;;;uncomment -iadc if realtime audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o outrg.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 4        ;quad
    0dbfs  = 1

    instr 1

    kleft init 1
    asig  vco2 .5, 220			;sawtooth
    idur = p3/(nchnls-1)
    knext init idur
    kpos init 0
    krate init 1/idur
    kbase init 0
    ktime timeinsts
    if ktime>=knext then
      kleft = kleft + 1
      knext = knext + idur
      kpos = 0
      kbase = ktime
    else
      kpos = (ktime-kbase)/idur
    endif
    printks "speaker %d position %f\n", 0, kleft, kpos
    a1,a2 pan2 asig, kpos
          outrg  kleft, a1, a2
    kpos = kbase/idur
    endin

    </CsInstruments>
    <CsScore>

    i 1 0 10
    e
    </CsScore>
    </CsoundSynthesizer>

Its output should include lines like these:

    speaker 1 position 0.000200
    speaker 1 position 0.000400
    speaker 1 position 0.000600
    .....
    speaker 1 position 1.000000
    speaker 2 position 0.000000
    speaker 2 position 0.000200
    ....
    speaker 2 position 0.999800
    speaker 3 position 0.000000
    speaker 3 position 0.000200
    ....
    speaker 3 position 0.999600
    speaker 4 position 0.000000
    .....

## Credits

Author: Gabriel Maldonado

New in version 5.06

Prev | Up | Next
outq | Home | outs1