mode
Prev | Orchestra Opcodes and Operators | Next

## mode

mode — A filter that simulates a mass-spring-damper system

## Description

Filters the incoming signal with the specified resonance frequency and quality factor. It can also be seen as a signal generator for high quality factor, with an impulse for the excitation. You can combine several modes to built complex instruments such as bells or guitar tables.

## Syntax

    aout mode ain, xfreq, xQ [, iskip]

## Initialization

iskip (optional, default=0) -- if non zero skip the initialisation of the filter.

## Performance

aout -- filtered signal

ain -- signal to filter

xfreq -- resonant frequency of the filter

| Warning
As this filter would become unstable if sr/xfreq < pi, the value of the xfreq is limited to sr/pi-sr/100 internally (e.g xfreq > 13596 Hz @ 44.1 kHz). The sr/100 term is because the filter while mathematically stable has a very large amplification as it approaches the unstable region.

xQ -- quality factor of the filter

The resonance time is roughly proportional to xQ/xfreq.

See Modal Frequency Ratios for frequency ratios of real instruments which can be used to determine the values of xfreq.

## Examples

Here is an example of the mode opcode. It uses the file mode.csd.

Example 585. Example of the mode opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    ; Audio out   Audio in    No messages
    -odac           -iadc     -d     ;;;RT audio I/O
    ; For Non-realtime ouput leave only the line below:
    ; -o moogvcf.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    ; Initialize the global variables.
    sr = 44100
    kr = 4410
    ksmps = 10
    nchnls = 2

    instr 1; 2 modes excitator

    idur init p3
    ifreq11 init p4
    ifreq12 init p5
    iQ11    init p6
    iQ12    init p7
    iamp    init ampdb(p8)
    ifreq21 init p9
    ifreq22 init p10
    iQ21    init p11
    iQ22    init p12

    ; to simulate the shock between the excitator and the resonator
    ashock  mpulse  3,0

    aexc1  mode ashock,ifreq11,iQ11
    aexc1 = aexc1*iamp
    aexc2  mode ashock,ifreq12,iQ12
    aexc2 = aexc2*iamp

    aexc = (aexc1+aexc2)/2

    ;"Contact" condition : when aexc reaches 0, the excitator looses
    ;contact with the resonator, and stops "pushing it"
    aexc limit aexc,0,3*iamp

    ; 2modes resonator

    ares1  mode aexc,ifreq21,iQ21
    ares2  mode aexc,ifreq22,iQ22

    ares = (ares1+ares2)/2

    display aexc+ares,p3
    outs  aexc+ares,aexc+ares

    endin

    </CsInstruments>
    <CsScore>

    ;wooden excitator against glass resonator
    i1 0 8  1000   3000  12  8  70  440   888   500  420

    ;felt against glass
    i1 4 8  80   188  8  3  70  440   888   500  420

    ;wood against wood
    i1 8 8  1000   3000  12  8  70  440  630   60  53

    ;felt against wood
    i1 12 8  80   180  8  3  70  440  630   60  53

    i1 16 8  1000   3000  12  8  70  440  888   2000  1630
    i1 23 8  80   180  8  3  70  440  888   2000  1630

    ;With a metallic excitator

    i1 33 8 1000  1800  1000  720  70   440   882  500  500
    i1 37 8 1000  1800  1000  850  70   440   630  60  53

    i1 42 8 1000  1800  2000  1720  70   440   442  500  500

    </CsScore>
    </CsoundSynthesizer>

## Credits

Original UDO and documentation/example by François Blanc

Opcode translation to C-code by Steven Yi

New in version 5.04

Audio rate parameters introduced in version 6.02

November 2013.

Prev | Up | Next
MixerClear | Home | modmatrix